{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Leht1"],"not_rendered":{"charts":0,"images":20,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Leht1","index":0,"n_rows":88,"n_cols":5,"rows_kept":88,"cut":false,"hidden":false,"merged":[[34,0,41,0],[75,0,76,0],[77,0,79,0],[80,0,84,0],[63,0,65,0],[66,0,67,0],[68,0,73,0],[26,1,28,1],[26,0,28,0],[60,0,62,0],[31,0,33,0],[52,0,55,0],[56,0,57,0],[58,0,59,0],[45,0,48,0],[49,0,51,0],[42,0,44,0],[11,0,12,0],[13,0,14,0],[15,0,16,0],[17,0,20,0],[29,0,30,0],[21,0,24,0]]}
[null,null,null,"Värskendatud: jaanuar 2022"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"allahindlus:",0]
["Vaade","Kood","Nimetus","Hind km-ta EUR","Hind km-ta EUR"]
[null,9018505,"Watts ruumitermostaat 24V, 15w, NC",20.715199999999999,{"$f":"IF($E$10>0,D12*(100%-$E$10),CLEAN(\"\"))","v":""}]
[null,9018515,"Watts ruumitermostaat 230V, 75w, NC",20.715199999999999,{"$f":"IF($E$10>0,D13*(100%-$E$10),CLEAN(\"\"))","v":""}]
[null,9018545,"Watts ruumitermostaat 24V, 15w, NC põrandaanduriga",29.68,""]
[null,9018555,"Watts ruumitermostaat 230V, 75w, NC põrandaanduriga",39.750500000000002,""]
[null,9018580,"Watts ruumitermostaat 24V, 15w, NC LCD ekraaniga",52.2,""]
[null,9018585,"Watts ruumitermostaat 230V, 75w, NC LCD ekraaniga",51.916400000000003,""]
[null,9018595,"Watts põhikontroller 24V 4 tsooni",64.553100000000001,""]
[null,9018605,"Watts põhikontroller 24V 6 tsooni",80.2179,""]
[null,9018635,"Watts põhikontroller 230V 4 tsooni",77.061400000000006,""]
[null,9018645,"Watts põhikontroller 230V 6 tsooni",91.656199999999998,""]
[null,9018615,"Watts põhikontrolleri laiendus 24V 4 tsooni",57.876300000000008,""]
[null,9018625,"Watts põhikontrolleri laiendus 24V 6 tsooni",64.5745,""]
[null,9018655,"Watts põhikontrolleri laiendus 230V 4 tsooni",66.521900000000002,""]
[null,9018665,"Watts põhikontrolleri laiendus 230V 6 tsooni",81.127399999999994,""]
[null,9018675,"Trafo Watts 230V / 24V, maksimaalselt 18 ajamile",44.24,""]
[null,9018680,"Watts nädalaprogrammkell 24V / 230V LCD ekraaniga",77.88,""]
[null,null,"Töötab ainult koos põhikontrolleriga.",0,""]
[null,null,"Võimalik juhtida kuni 2 eraldiseisvat tsooni",0,""]
[null,2050600,"Watts ajam 230V M30 NC",27.84,""]
[null,2050601,"Watts ajam 24V M30 NC",27.84,""]
[null,215115,"Kaitseklapp 1/2\" 1,5bar Küttele",7.3,""]
[null,215125,"Kaitseklapp 1/2\" 2,5bar Küttele",7.3,""]
[null,215130,"Kaitseklapp 1/2\" 3bar Küttele",7.3,""]
[null,"0216104","Kaitseklapp 1/2\" 4bar Tarbeveele",7.3,""]
[null,"0216106","Kaitseklapp 1/2\" 6bar Tarbeveele",7.3,""]
[null,"0216108","Kaitseklapp 1/2\" 8.0 bar Tarbeveele",7.3,""]
[null,"0216110","Kaitseklapp 1/2\" 10,0 bar Tarbeveele",7.3,""]
[null,217204,"Kaitseklapp 3/4\" 4,0bar Tarbeveele",12.24,""]
[null,"0217206","Kaitseklapp 3/4\" 6,0bar Tarbeveele",12.24,""]
[null,217208,"Kaitseklapp 3/4\" 8,0bar Tarbeveele",12.24,""]
[null,"0217210","Kaitseklapp 3/4\" 10,0bar Tarbeveele",12.24,""]
[null,"0217215","Kaitseklapp 3/4\" 1,5bar Küttele",12.24,""]
[null,217625,"Kaitseklapp 3/4\" 2,5bar Küttele",12.24,""]
[null,"0217630","Kaitseklapp 3/4\" 3,0bar Küttele",12.24,""]
[null,"0218304","Kaitseklapp 1\" 4,0bar Tarbeveele",27.12,""]
[null,"0218306","Kaitseklapp 1\" 6,0bar Tarbeveele",27.12,""]
[null,"0218308","Kaitseklapp 1\" 8,0bar Tarbeveele",27.12,""]
[null,"0218310","Kaitseklapp 1\" 10,0bar Tarbeveele",27.12,""]
[null,"0218325","Kaitseklapp 1\" 2,5bar Küttele",27.12,""]
[null,218330,"Kaitseklapp 1\" 3,0bar Küttele",27.12,""]
[null,"0218615","Kaitseklapp 1\" 1,5bar Küttele",27.12,""]
[null,"0219404","Kaitseklapp 1 1/4\" 4,0bar Tarbeveele",56.89,""]
[null,"0219406","Kaitseklapp 1 1/4\" 6,0bar Tarbeveele",56.89,""]
[null,"0219408","Kaitseklapp 1 1/4\" 8,0bar Tarbeveele",56.89,""]
[null,"0219410","Kaitseklapp 1 1/4\" 10,0bar Tarbeveele",56.89,""]
[null,"0219425","Kaitseklapp 1 1/4\" 2,5bar Küttele",56.89,""]
[null,"0219430","Kaitseklapp 1 1/4\" 3,0bar Küttele",56.89,""]
[null,251410,"Õhutusklapp 0251410 WATTS sirge 1/2\"",7.48,""]
[null,254015,"Õhutusklapp 0254015 WATTS nurkne 1/2\"",10.06,""]
[null,301040,"Bi-metall termomeeter 63mm 0-120 1/2\" L50",4.47,""]
[null,301100,"Bi-metall termomeeter 63mm 0-120 1/2\" L100",7.85,""]
[null,308060,"Bi-metall pinnatermomeeter 63mm 0-120  1/2\" L50, vedruga",6.53,""]
[null,"0318206","Manomeeter 63mm 0-6bar 1/4\" alt",6.1,""]
[null,"0322206","Manom. 100mm 0-6bar 1/2\" alt 0322206",11.62,""]
[null,322210,"Manom. 100mm 0-10bar 1/2\" alt 0322210",12.03,""]
[null,"0332006","Termo-manomeeter tagantühendus 1/2\" 0-6bar",20.49,""]
[null,333006,"Termo-manomeeter altühendus 1/2\" 0-6bar",20.49,""]
[null,502515,"Reg. rõhualandusventiil 1/2\"  DRV15/N",55.35,""]
[null,"0502520","Reg. rõhualandusventiil 3/4\"  DRV20/N",65.31,""]
[null,"0502525","Reg. rõhualandusventiil 1\"  DRV25/N",91.78,""]
[null,"0502532","Reg. rõhualandusventiil 11/4\"  DRV32/N",126.26,""]
[null,"0502540","Reg. rõhualandusventiil 11/2\"  DRV40/N",243.12,""]
[null,"0502550","Reg. rõhualandusventiil 2\"  DRV50/N",276.32,""]
[null,606112,"Katlagrupp 3/4\" seinale GAG/MR 20/E",63.25,""]
[null,"1071316","Eurokoonus Watts 16 x 3/4\"",2.5299999999999998,""]
[null,1071320,"Eurokoonus Watts 20 x 3/4\"",2.5299999999999998,{"$f":"IF($E$10>0,D77*(100%-$E$10),CLEAN(\"\"))","v":""}]
[null,"1701043","Tsirkulatsiooni pump HP43 WATTS",80.09,""]
[null,"1701063","Tsirkulatsiooni pump HP63 WATTS",95.56,""]
[null,"1701163","Tsirkulatsiooni pump 2\" HP63 WATTS",142.97999999999999,""]
[null,"M063-10-A","Manom. 63mm 0-10bar 1/4\" alt 0318210",5.81,""]
[null,"M063-10-T","Manom. 63mm 0-10bar 1/4\" tagant 0316210",5.81,""]
[null,"M063-6-T","Manom. 63mm 0-6bar 1/4\" tagant 0316206",5.81,""]
[null,"M100-16A","Manom. 100mm 0-16bar 1/2\" alt 0322216",11.62,""]
[null,"M100-25A","Manom. 100mm 0-25bar 1/2\" alt 0322225",11.62,""]
[]
["Küttemaailm OÜ jätab endale õiguse hindasid muuta ilma eelnevalt ette teatamata."]
["Kehtivat hinnakirja saab kontrollida aadressil www.kyttemaailm.ee"]